C Controller - GUIs 

Page / - last modified by Soeren Domroes on 2025/01/30 12:05 

GUIs 
last modified by Soeren Domroes
on 2025/01/30 12:05

Table of Contents

The GUIs communicate via TCP and JSON with the railway controller. Because of this platform in dependency, it's easily possible to connect multiple different GUI-clients to the controller.
We implemented two different clients, the first running on the common (desktop) JVM and the second running on android based devices.
Desktop
AndroidAndroid